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liquid-cooled, in-line Allison engine. This is an
improved version of the P-40D, called “Kitty-
hawk” by the R.A.F. Span 37’ 4, Length 31" 9”.

Identification

Low-wing monoplane. Very slight sweepback on

P-40E

leading edge of wing, trailing edge swept for- BILL OF MATERIALS
ward to rounded tips. Small “knees” for housing Fuselage ......... Yx1Vax5% U.S. ARMY FIGHTER
Wing ............ 15X 1%x6% FINAL ASSEMBLY

retracted landing gear struts under wings near

Tail ... ... ... Hx1%x3% ”
fuselage. Long nose with row of exhausts on Belly Block .. ....... VexVax 1% SPAN 6-7/32 | SERIAL NO. A-9 |DATE 2-16-42
each side and large radiator below. Knee Blocks ........ = thick
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